for graphics version only PLOT

__________________________________________________________________________________

PLOT (A4, DASH, DEVICE= name of printer , FILE= name of file , HEIGHT = height of characters ,

HIRES, LANDSCAP, MIN= y axis minimum , MAX= y axis maximum ,

ORIGIN, PORT RAIT , PREVIEW, T IT LE=’ text string to be used as title ’, WIDT H) ;

__________________________________________________________________________________

Function:

P LOT p r o d uces a p lo t of one or more series versus the observation number (usuallyin units of time). T he series ar e p lotted on the vertical axis and time on the horizontal axis. T he plot maybe printed as well as displayed if a hardcopy d evicesuchasaLaserjetordotmatrixprinteris available. T his section describes the graphics version of PLOT , which is availableonlyforDOS/WinandMacintoshversionsorTSP.Forotherversions,seethenon-graphics PLOTcommand .

Usage:

PLOT isfollowed byasingleseriesname,oralistofseriesnames.Ontheplot,theserieswillbedifferentiated bycolor s o rthestyleofthelinesused to plotthem.Parametersto controltheappearanc e and printing of the plot maybe included in parentheses following the word PLOT .

T he graph will be displayed on the screen; if a DEVICE= is specified, a prompt is also displayed which instructs you to type "P" if you wish to print the graph. If you type anything else, the graph will not be printed; this is useful if yo u decide you do not like its appearance after you have seen the screen.

If there are anyobservations with missing data, there will be breaks in the plotted lines.

Options:

(DOS/Win only) A4/ NOA4 specifies A4 paper size. Available for DEVICE=LJ3 or POST SCRIPT only.

D ASH/ NODASH specifieswhetherthelinesfordifferentseriesonthescree n are to be distinguished byusing different d ashpatterns(ofwhichthereareseven).Thedefaultisno dashes(justcolor)onthescreenand dashesonprinted output.

(D OS/Win only) DEVICE =CHAR or EPSON or LJ2 or LJ3 or LJET or LJPLUS or LJR75 or LJR100 or LJR150 o r

LJ R3 0 0 o r POST SCRI or PS specifies the hardcopydevice to be used for printer output. LJ means HP LaserJet o r c ompatible,EPSONisEPSONdotmatrixorcompatible,POSTSCRIand PSarePostcri pt output, and CHAR is the old line printer output (characters instead of graphics). T he LJ suffixes specifymodels of the printer and the LJR suffixes s pecifytheresolutionoftheLaserJetprinter directly, rather than giving the printer type. T he default resolutions for the

L JET,LJPLUS,and LJ2 printersare100,150,and 300 respectively.Notetha t larger resolutions implylarger file sizes and printing times.

( DOS/Win only) FILE =thenameofafileto whichthegraphicsimageist o be written. T his file can be printed later; for example, if you are running under DOS and your printer device is LPT 1, print the plot with the command copy/b file LPT 1:

(DOS/Win only) HEIGHT = letter height in inches. T he default*is .25. Values in the range (0,1] are valid.

(DOS/Win only) HIRES/ NOHIRES controlshowgraphsareprintedin batchmode(whenPREVIEW isnotbeingused) .

N ormally(NOHIRES),graphsarepri nted in character mode to the batch output file. When the HIRES option is used, the patched DEVICE= and FILE= will be used; usuallythis will send a page to LPT 1 for each graph.

PLOT for graphics version only

( DOS/Win only) LANDSCAP /PORT RAIT specifies the orientation of the plot. On the Mac, specifythis option in the dialog box.

M IN = minimumvalue for the y-axis. T his value must be less than or equal to the minimumvalue in the data.

M AX = maximumvalue for the y-axis. T his value must be greater than or equal to the maximumvalue in the data.

ORIGIN/ NOORIGIN causes a horizontal line to be drawn starting at zero on the vertical axis.

P REVIEW /NOPREVIEspecifieswhetherthegraphisto beshownonthescreenbeforepri nting or saving. T he default is PREVIEW for interactive use and NOPREVIE for batch use.

TITLE =’a string which will be printed across the top of the graph’.

(MA C o n ly ) WIDT H/ NOWIDTH specifies whether varying width sizes are to be used to distinguish the line s corresponding to different series on the graph.

* Fo r co nvenien ce, the DEVICE=, FILE= AND HEIGHT = options of PLOT that you set are retained in the nex t

P LOT(s)orGRAPH(s)untiltheyareoverridenexplicitly.Theymayalso besetina LOGIN.T SP file bynot specifying anyseries to plot. For example:

PLOT (DEV=LJ3, HEIGHT =.2) ;

Example:

T he following example plots the graph shown on the following page:

OPT IONS CRT NODAT E;

NAME ALMONS; ? ALMON AND SHILLER LAGS

FREQ Q;

SMPL 53:1 67:4;

LOAD;

PLOT (PORT ,PREV,DEV=LJ3,FILE=’ALMON.PLT ’,T IT LE=’ALMON DAT A’) EXPEND APPROP;

END;

NOPRINT ;

LOAD expend approp; ? ORIGINAL ALMON DAT A FROM MADDALA, P. 370

2072 1660 2077 1926 2078 2181 2043 1897 2062 1695 2067 1705 1964 1731 1981 2151

...

5715 5412 5637 5465 5383 5550 5467 5465;

Output:

In the high resolution screen mode, PLOT puts time (the observations index) on the horizontal axis and differentiates t he series bya line type (dashes in the DOS/Win version, line width in the PC/MAC version). On a color monitor, the lines will have different colors. Check your installation disk for more Graphics documentation.

for graphics version only PLOT